**NCTS-POS12（4G／128G）**

|  |  |
| --- | --- |
| **Configuration（MODEL: NCTS-POS12）** | |
| Cabinet size | 365mm(W)\*340mm(L)\*280mm(H) |
| Main Board | Industrial POS motherboard- Intel 1900 |
| CPU | Dual-core Processor |
| Memory | DDR3 4G |
| Hard Disk | 128G SSD |
| Power | 250W/220V/110V ATX Power supply |
| Interface | 1 PS/2 mouse & 1 PS/2 keyboard，  1 Parallel port，  6 USB ports，  1 LAN port，  1 VGA port，  1 Serial port  1 Audio output  1 Audio input |
| Monitor | 15'' TOUCH TFT LCD ELO5 Resistive touch panel--Resolution:1024\*768 |
| Printer(optional) | 58mm thermal printer  (Optional:76mm dot-matrix printer, or 80mm thermal with auto-cutter printer) |
|  |  |
| POS keyboard(optional) | KB-101 keyboard  (Optional keyboard with magcard reader track2+3, or programmable keyboard with magcard reader track2+3) |
| Cash drawer(optional) | Cash Drawer |
| Bar code scanner(optional) | CCD bar code scanner or Laser bar code scanner/2D Scanner |
| Customer display | LED 8N,8digits |
| Magcard reader, writer(optional) | Track1+2+3,USB port or PS2 port or Serial port |
| IC card reader, writer(optional) | Contact or Contactless |
| Password Keyboard（optional） | With LED or without LED |